**TS8132 UPG Update Guide**

1. Put TS8132.UPG file on root of a USB(FAT32) stick

2. Power on the TS8132 to display “Hello”

3. Make Sure subwoofer connected to the Soundbar

4. If the Sbar is in USB Mode(You can insert USB with MP3 file, at USB source, check it whether it can play music), just skip to step 5, if you Sbar is in adb Mode, do “Long press the Source and BlueTooth buttons about 5s until you see USB Mode displayed”

5. Insert the USB stick and wait for UPGxx displayed

6. Wait until update is done(You can see UPGOK displayed) and display shows START when completed

**Check Version**

1. Power on the TS8132 to display “Hello”
2. Short Press Power key on panel button or Ir button, Sbar will show “Sleep”
3. Then long press IR “OK” key 5s, VFD will show “Wait”
4. Then VFD will show “Version”, press IR “OK” key, it will show Version, press IR “Volume Down“ key, it will jump to show other module version. The M xxx is mean the main version.
5. You can short press “Power“ key to exit check version, short press “Power“ key again to go back normal work mode.

This time, “Volume UP” key is back to previous action

**Factory Reset**

1. Power on the TS8132 to display “Hello”
2. Short Press Power key on panel button or Ir button, Sbar will show “Sleep”
3. Then long press IR “OK” key 5s, VFD will show “Wait”
4. Then VFD will show “Version”, press IR “Volume Down” key to go to “FACTORY RESET”, then press IR “OK” key, it will show “YES”, Press IR “OK” key, it will do factory reset and will reboot.

This time, “Volume UP” key is back to previous action