**TS8212 USB Disk Upgrade Instructions**

**Version: V107**

Filename: **TS8212.UPG** (Unzip “TS8212 20211105 VER 107\_107\_05\_12\_20\_10\_082\_082\_02.rar”)

Release Date: **11/05/2021**

|  |  |
| --- | --- |
| Release Notes: | |
| 1 | Add the “DO NOT SUPPORT” prompt function on Soundbar LED Display when playing DTS audio format. |
| 2 | Optimize some scenarios where the wireless module interferes with the BT module (automatically pairing after power-on) |
| 3 | Improve BT module upgrade |
| 4 | Improve the silent output problem in some operation scenarios under HMDI IN/ARC SRC" |

## **How to upgrade by USB Disc**

Requirements:

* TCL Sound Bar
* Computer connected to the Internet
* A USB flash device formatted in FAT/FAT32 with at least 100MB of free space.
  + Remove all files and folders from the USB flash device (it should be empty).

Upgrade Procedure:

* Power on by pressing the” **Power**” button on the Sound Bar
* Unzip “TS8212 20XXXXXX VER XXX\_XXX\_XX\_XX\_XX\_XX\_XXX\_XXX\_XX”, and move or copy the upgrade file **TS8212.UPG** inside the root directory of the USB flash device.
* Plug the USB flash device into the Sound Bar
* “**WAIT”** will be shown during the upgrade. Plug out the USB flash device when the white LED is on.
* Press the “**Power**” button to power on the Sound Bar and the upgrade is done.

**Remark:**  Pls don’t remove the USB flash device or power off the soundbar during the software upgrade processing, or it will cause the upgrade to fail and the soundbar to break.